(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (grid_origin 104.9865 80)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(U1-CV)")
  (net 2 "0")
  (net 3 "Net-(D1-K)")
  (net 4 "Net-(D1-A)")
  (net 5 "VCC")
  (net 6 "Net-(Q1-G)")
  (net 7 "Net-(U1-Q)")
  (net 8 "Net-(U1-THR)")
  (net 9 "Net-(D2-A)")
  (net 10 "Net-(J1-Pin_3)")
  (footprint "Diode_THT:D_DO-34_SOD68_P7.62mm_Horizontal" (layer "F.Cu")
    (at 125.7 52.1 180)
    (descr "Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf")
    (tags "Diode DO-34_SOD68 series Axial Horizontal pin pitch 7.62mm  length 3.04mm diameter 1.6mm")
    (property "Sheetfile" "driver_led_kloeckner.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "SUBCKT")
    (property "Sim.Library" "/home/mk/dox/fiuba/86.70/driver_led_integrador/modelos_spice/1N4148.lib")
    (property "Sim.Name" "1N4148")
    (property "Sim.Pins" "1=1 2=2")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D2" (at 4.245 -0.03) (layer "F.SilkS"))
    (fp_text value "4148" (at 6.7365 2) (layer "F.Fab"))
    (fp_text user "K" (at -2.1 -0.1) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.038 0) (layer "F.Fab"))
    (fp_text user "K" (at -2.1135 -0.1) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-34_SOD68_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 130.51 49 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "driver_led_kloeckner.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 3.9465 -0.05 180) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.96 -0.05 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "VCC") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_Altech_AK300-3_P5.00mm" (layer "F.Cu")
    (at 136.1865 65.5 90)
    (descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
    (tags "Altech AK300 terminal block pitch 5.0mm")
    (property "Sheetfile" "driver_led_kloeckner.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Enable" "0")
    (property "ki_description" "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J1" (at -1 -4.5 180) (layer "F.SilkS") hide)
    (fp_text value "Bornera" (at 4.95 7.3 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 5 -2 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.98 3.96) (drill 1.32) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J1-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "2" thru_hole oval (at 5 0 90) (size 1.98 3.96) (drill 1.32) (layers "*.Cu" "*.Mask")
      (net 2 "0") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 10 0 90) (size 1.98 3.96) (drill 1.32) (layers "*.Cu" "*.Mask")
      (net 5 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KIPRJMOD}/pwm_driver_3d_models/screw-terminal-dg-301-5mm-1.snapshot.1/dg-301-5_0.step"
      (offset (xyz -2.5 -3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (at 109.2365 72)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "driver_led_kloeckner.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 2.55 0) (layer "F.SilkS"))
    (fp_text value "10nF" (at 2.5 2.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(U1-THR)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 118.94 68.1)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "driver_led_kloeckner.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "R")
    (property "Sim.Pins" "1=+ 2=-")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 3.96 0.05) (layer "F.SilkS"))
    (fp_text value "46k" (at 9.81 0.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0.05) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(U1-Q)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Q1-G)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (at 128.4865 60 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "driver_led_kloeckner.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 2.5 -0.18 90) (layer "F.SilkS"))
    (fp_text value "10nF" (at -3.05 -0.0135 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(U1-CV)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-34_SOD68_P7.62mm_Horizontal" (layer "F.Cu")
    (at 118.03 54.5)
    (descr "Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf")
    (tags "Diode DO-34_SOD68 series Axial Horizontal pin pitch 7.62mm  length 3.04mm diameter 1.6mm")
    (property "Sheetfile" "driver_led_kloeckner.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "SUBCKT")
    (property "Sim.Library" "/home/mk/dox/fiuba/86.70/driver_led_integrador/modelos_spice/1N4148.lib")
    (property "Sim.Name" "1N4148")
    (property "Sim.Pins" "1=1 2=2")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D1" (at 4.245 -0.03) (layer "F.SilkS"))
    (fp_text value "4148" (at 3.3785 1.5) (layer "F.Fab") hide)
    (fp_text user "K" (at -1.8715 -0.05) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.038 0) (layer "F.Fab"))
    (fp_text user "K" (at -1.8715 -0.05) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.5 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-34_SOD68_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Alps_RK163_Single_Horizontal" (layer "F.Cu")
    (at 108.9865 56.4)
    (descr "1110U1Q 1110TNP 1110U2A 1110U0Q Potentiometer, horizontal, Alps RK163 Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk16/rk16.pdf")
    (tags "Potentiometer horizontal Alps RK163 Single")
    (property "Sheetfile" "driver_led_kloeckner.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "R")
    (property "Sim.Params" "r=50k pos=0.75")
    (property "Sim.Pins" "1=r0 2=wiper 3=r1")
    (property "Sim.Type" "POT")
    (property "ki_description" "Potentiometer, US symbol")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "RV1" (at 4.5 12.5 180) (layer "F.SilkS") hide)
    (fp_text value "50k" (at 5.3635 5.25 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.3135 5.1 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 3 3) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D2-A)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 5 180) (size 3 3) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(U1-THR)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 10 180) (size 3 3) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pinfunction "3") (pintype "passive"))
    (model "${KIPRJMOD}/pwm_driver_3d_models/alpha-rv16af-20-1.snapshot.9/RV16AF-20.step"
      (offset (xyz 7 -5 12.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (at 117.9865 64.9 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "driver_led_kloeckner.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "SUBCKT")
    (property "Sim.Library" "/home/mk/dox/fiuba/86.70/driver_led_integrador/modelos_spice/555.lib")
    (property "Sim.Name" "555b")
    (property "Sim.Pins" "1=1 2=2 3=3 4=4 5=5 6=6 7=7 8=8")
    (property "ki_description" "Precision Timers, 555 compatible,  PDIP-8")
    (property "ki_keywords" "single timer 555")
    (attr through_hole)
    (fp_text reference "U1" (at 3.95 2.7135 90) (layer "F.SilkS"))
    (fp_text value "NE555P" (at 3.8 4.5135 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.95 2.6635 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "0") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(U1-THR)") (pinfunction "TR") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(U1-Q)") (pinfunction "Q") (pintype "output"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "VCC") (pinfunction "R") (pintype "input"))
    (pad "5" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(U1-CV)") (pinfunction "CV") (pintype "input"))
    (pad "6" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(U1-THR)") (pinfunction "THR") (pintype "input"))
    (pad "7" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-A)") (pinfunction "DIS") (pintype "input"))
    (pad "8" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 125.25 71.5 180)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "driver_led_kloeckner.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "SUBCKT")
    (property "Sim.Library" "/home/mk/dox/fiuba/86.70/driver_led_integrador/modelos_spice/IRF1407.spi")
    (property "Sim.Name" "irf1407")
    (property "Sim.Pins" "1=1 2=2 3=3")
    (property "ki_description" "N-MOSFET transistor, drain/source/gate")
    (property "ki_keywords" "transistor NMOS N-MOS N-MOSFET simulation")
    (attr through_hole)
    (fp_text reference "Q1" (at -4.0135 -1.2 90) (layer "F.SilkS") hide)
    (fp_text value "IRF1407" (at 2.65 -4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.65 -2.15) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J1-Pin_3)") (pinfunction "D") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Q1-G)") (pinfunction "G") (pintype "input"))
    (pad "3" thru_hole oval (at 5.08 0 180) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "0") (pinfunction "S") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "/home/mk/dox/fiuba/86.70/driver_led_integrador/TO-220-3_Vertical_trimmed_legs_colored.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_circle (center 108 77) (end 109.5 77)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 108 48) (end 109.5 48)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 137 48) (end 138.5 48)
    (fill none) (layer "Edge.Cuts"))
  (gr_rect (start 104.9865 45) (end 139.9865 80)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 137 77) (end 138.5 77)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "max\n18V" (at 138.7 69.4 90) (layer "F.SilkS"))
  (gr_text "PWM\nDriver" (at 114.75 46.1 180) (layer "F.SilkS"))
  (gr_text "-PWM  -   +" (at 132 70.9 90) (layer "F.SilkS"))
  (gr_text "kloeckner.com.ar" (at 111.5365 78.75) (layer "F.SilkS"))
  (zone (net 2) (net_name "0") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 104.95 45)
        (xy 104.95 77.7)
        (xy 107.3 80.05)
        (xy 138 80.05)
        (xy 140 78.05)
        (xy 140 47.35)
        (xy 137.65 45)
        (xy 107.05 45)
        (xy 105 47.05)
        (xy 105 45.05)
      )
    )
  )
)
