(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 135.62 86 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R4"
			(at 3.81 -0.035 0)
			(layer "F.SilkS")
		)
		(property "Value" "220k"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(JP2-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U1--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 146.81 86 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R5"
			(at 3.81 -0.035 0)
			(layer "F.SilkS")
		)
		(property "Value" "20k"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(JP2-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 128 82.5)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R3"
			(at 3.81 -0.035 0)
			(layer "F.SilkS")
		)
		(property "Value" "20k"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U1--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 139.75 93.775 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "JP2"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Jumper_2_Small_Bridged"
			(at 0 4.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 2-pole, small symbol, bridged"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/pin_header_socket"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(JP2-A)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(JP2-B)")
			(pinfunction "B_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 116.69 86)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R1"
			(at 3.81 -0.035 0)
			(layer "F.SilkS")
		)
		(property "Value" "180k"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U3--)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(JP1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x03_P3.50mm_Vertical"
		(layer "F.Cu")
		(at 111 101.1675)
		(descr "Terminal Block 4Ucon ItemNo. 10694, vertical (cable from top), 3 pins, pitch 3.5mm, size 11.5x8.3mm, drill diameter 1.3mm, pad diameter 2.6mm, http://www.4uconnector.com/online/object/4udrawing/10694.pdf")
		(tags "THT Terminal Block 4Ucon ItemNo. 10694 vertical pitch 3.5mm size 11.5x8.3mm drill 1.3mm pad 2.6mm")
		(property "Reference" "J2"
			(at 3.5 3.0825 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 3.5 5.72 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "terminal_block/4Ucon"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.5 3.45 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.096154)
			(net "GND")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.5 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+24V")
			(pinfunction "Pin_2_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 7 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "-24V")
			(pinfunction "Pin_3_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d_models/KF350-3p.step"
			(offset
				(xyz -1.75 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 105.69 95.5)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R0"
			(at 3.81 -0.035 0)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(attr through_hole board_only)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "-24V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "-24V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
		(layer "F.Cu")
		(at 119.25 89.5)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm diameter 4.3mm width 1.9mm Capacitor")
		(property "Reference" "C1"
			(at 2.5 0.065 0)
			(layer "F.SilkS")
		)
		(property "Value" "22n"
			(at 2.5 2.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "capacitor/THT/other"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U3--)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(JP1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
		(layer "F.Cu")
		(at 154.25 77.5 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm diameter 4.3mm width 1.9mm Capacitor")
		(property "Reference" "C2"
			(at 2.5 0.065 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2n"
			(at 2.5 2.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "capacitor/THT/other"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 116.69 82.5)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R2"
			(at 3.81 -0.035 0)
			(layer "F.SilkS")
		)
		(property "Value" "180k"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(JP1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 123.5 94.725)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "JP1"
			(at 0 5.275 0)
			(layer "F.SilkS")
		)
		(property "Value" "Jumper_2_Small_Bridged"
			(at 0 4.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 2-pole, small symbol, bridged"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/pin_header_socket"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(JP1-A)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(JP1-B)")
			(pinfunction "B_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 146.38 90.75)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U2"
			(at 3.805 4.06 0)
			(layer "F.SilkS")
		)
		(property "Value" "TL081"
			(at 3.81 9.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl081.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single JFET-Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/DIP/legacy"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "3" "2" "7" "4" "8" "1" "5" "6")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 90)
			(layer "F.Fab")
		)
		(point
			(at 150.19 94.56)
			(size 1.27)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net "unconnected-(U2-NULL-Pad1)")
			(pinfunction "NULL_1")
			(pintype "input+no_connect")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/Vout")
			(pinfunction "-_2")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-+)")
			(pinfunction "+_3")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "-24V")
			(pinfunction "V-_4")
			(pintype "power_in")
		)
		(pad "5" thru_hole circle
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(U2-NULL-Pad5)")
			(pinfunction "NULL_5")
			(pintype "input+no_connect")
		)
		(pad "6" thru_hole circle
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/Vout")
			(pintype "output")
		)
		(pad "7" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+24V")
			(pinfunction "V+_7")
			(pintype "power_in")
		)
		(pad "8" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(U2-NC-Pad8)")
			(pinfunction "NC_8")
			(pintype "no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 139.19 82.5)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R6"
			(at 3.81 -0.035 0)
			(layer "F.SilkS")
		)
		(property "Value" "30k"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U2-+)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 127.695 92.69)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U1"
			(at 3.81 4.06 0)
			(layer "F.SilkS")
		)
		(property "Value" "TL081"
			(at 3.81 9.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl081.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single JFET-Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/DIP/legacy"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "3" "2" "7" "4" "8" "1" "5" "6")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 90)
			(layer "F.Fab")
		)
		(point
			(at 131.505 96.5)
			(size 1.27)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net "unconnected-(U1-NULL-Pad1)")
			(pinfunction "NULL_1")
			(pintype "input+no_connect")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U1--)")
			(pinfunction "-_2")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(JP1-B)")
			(pinfunction "+_3")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "-24V")
			(pinfunction "V-_4")
			(pintype "power_in")
		)
		(pad "5" thru_hole circle
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(U1-NULL-Pad5)")
			(pinfunction "NULL_5")
			(pintype "input+no_connect")
		)
		(pad "6" thru_hole circle
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(JP2-A)")
			(pintype "output")
		)
		(pad "7" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+24V")
			(pinfunction "V+_7")
			(pintype "power_in")
		)
		(pad "8" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(U1-NC-Pad8)")
			(pinfunction "NC_8")
			(pintype "no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 104.63 84.88)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U3"
			(at 3.805 3.81 0)
			(layer "F.SilkS")
		)
		(property "Value" "TL081"
			(at 3.81 9.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl081.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single JFET-Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "package/DIP/legacy"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "3" "2" "7" "4" "8" "1" "5" "6")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 90)
			(layer "F.Fab")
		)
		(point
			(at 108.44 88.69)
			(size 1.27)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net "unconnected-(U3-NULL-Pad1)")
			(pinfunction "NULL_1")
			(pintype "input+no_connect")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U3--)")
			(pinfunction "-_2")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/Vin")
			(pinfunction "+_3")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "-24V")
			(pinfunction "V-_4")
			(pintype "power_in")
		)
		(pad "5" thru_hole circle
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(U3-NULL-Pad5)")
			(pinfunction "NULL_5")
			(pintype "input+no_connect")
		)
		(pad "6" thru_hole circle
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U3--)")
			(pintype "output")
		)
		(pad "7" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+24V")
			(pinfunction "V+_7")
			(pintype "power_in")
		)
		(pad "8" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(U3-NC-Pad8)")
			(pinfunction "NC_8")
			(pintype "no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal"
		(layer "F.Cu")
		(at 140.42 76.58)
		(descr "http://www.farnell.com/datasheets/612848.pdf")
		(tags "BNC Amphenol Horizontal")
		(property "Reference" "J3"
			(at 0 -5.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at 0 6 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0)
			(size 1.6 2.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/Vout")
			(pinfunction "In_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -5.08 -5.08)
			(size 3.5 7)
			(drill 2.01)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Ext_2")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -2.54 0)
			(size 1.6 2.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Ext_2")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5.08 -5.08)
			(size 3.5 7)
			(drill 2.01)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Ext_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal"
		(layer "F.Cu")
		(at 117.58 76.5)
		(descr "http://www.farnell.com/datasheets/612848.pdf")
		(tags "BNC Amphenol Horizontal")
		(property "Reference" "J1"
			(at 0 -5 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at 0 6 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0)
			(size 1.6 2.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/Vin")
			(pinfunction "In_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -5.08 -5.08)
			(size 3.5 7)
			(drill 2.01)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Ext_2")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -2.54 0)
			(size 1.6 2.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Ext_2")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5.08 -5.08)
			(size 3.5 7)
			(drill 2.01)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Ext_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
		(layer "F.Cu")
		(at 150.5 82.5 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm diameter 4.3mm width 1.9mm Capacitor")
		(property "Reference" "C3"
			(at 2.5 0.065 90)
			(layer "F.SilkS")
		)
		(property "Value" "47n"
			(at 2.5 2.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "capacitor/THT/other"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "board.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/Vout")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 99 63)
		(end 159 108)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 103.581139 67.581139)
		(end 104.081139 66.081139)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 103.581139 103.418861)
		(end 104.081139 101.918861)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 154.418861 67.581139)
		(end 154.918861 66.081139)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 154.418861 103.418861)
		(end 154.918861 101.918861)
		(fill no)
		(layer "Edge.Cuts")
	)
	(zone
		(net "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
		)
		(polygon
			(pts
				(xy 99 63) (xy 159 63) (xy 159 108) (xy 99 108)
			)
		)
	)
	(embedded_fonts no)
)
