(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(grid_origin 104.9865 80)
		(pcbplotparams
			(layerselection 0x0001020_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "../pwm_driver_fabrication_files/")
		)
	)
	(net 0 "")
	(net 1 "Net-(U1-CV)")
	(net 2 "Net-(D1-K)")
	(net 3 "Net-(D1-A)")
	(net 4 "VCC")
	(net 5 "Net-(U1-THR)")
	(net 6 "Net-(D2-A)")
	(net 7 "Net-(J1-Pin_3)")
	(net 8 "GND")
	(net 9 "Net-(Q1-G)")
	(footprint "Diode_THT:D_DO-34_SOD68_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 121.8015 47.5 180)
		(descr "Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf")
		(tags "Diode DO-34_SOD68 series Axial Horizontal pin pitch 7.62mm  length 3.04mm diameter 1.6mm")
		(property "Reference" "D2"
			(at 4.245 -0.03 0)
			(layer "F.SilkS")
		)
		(property "Value" "4148"
			(at 6.7365 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_THT:D_DO-34_SOD68_P7.62mm_Horizontal"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "SUBCKT"
			(at 252.303 102.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "${KIPRJMOD}/pwm_driver_spice_simulation_models/1N4148.lib"
			(at 252.303 102.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "1N4148"
			(at 252.303 102.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=1 2=2"
			(at 252.303 102.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "pwm_driver_kicad.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at -1.935 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 4.038 0 0)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at -1.685 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.5 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(D1-A)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.5 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-34_SOD68_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 132.9865 49.5 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 3.9465 -0.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 2.26 -1.5 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pwm_driver_kicad.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.96 -0.05 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(D1-A)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(at 125.4065 76.5)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q1"
			(at 2.54 -5 0)
			(layer "F.SilkS")
		)
		(property "Value" "IRF540"
			(at 2.54 2.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-manual.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "SUBCKT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=1 2=2 3=3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "pwm_driver_spice_simulation_models/irf540.lib"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "irf540"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "pwm_driver_kicad.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pin_3)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/pwm_driver_3d_models/TO-220-3_Vertical_trimmed_legs.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Altech_AK300-3_P5.00mm"
		(layer "F.Cu")
		(at 136.1865 65.5 90)
		(descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
		(tags "Altech AK300 terminal block pitch 5.0mm")
		(property "Reference" "J1"
			(at -1 -4.5 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Bornera"
			(at 4.95 7.3 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TerminalBlock:TerminalBlock_Altech_AK300-3_P5.00mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "Root")
		(sheetfile "pwm_driver_kicad.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5 -2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0 90)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 10 0 90)
			(size 1.98 3.96)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/pwm_driver_3d_models/terminal-block/terminal-block.step"
			(offset
				(xyz 5 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
		(layer "F.Cu")
		(at 109.9865 73)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
		(property "Reference" "C2"
			(at 2.55 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.5 2.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pwm_driver_kicad.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U1-THR)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
		(layer "F.Cu")
		(at 128.4865 58.5 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
		(property "Reference" "C1"
			(at 2.5 -0.18 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at -3.05 -0.0135 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pwm_driver_kicad.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(U1-CV)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 125.7965 70 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 3.81 -1.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pwm_driver_kicad.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(Q1-G)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-34_SOD68_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 114.1715 51)
		(descr "Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf")
		(tags "Diode DO-34_SOD68 series Axial Horizontal pin pitch 7.62mm  length 3.04mm diameter 1.6mm")
		(property "Reference" "D1"
			(at 4.245 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4148"
			(at 3.3785 1.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Diode_THT:D_DO-34_SOD68_P7.62mm_Horizontal"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "SUBCKT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "${KIPRJMOD}/pwm_driver_spice_simulation_models/1N4148.lib"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "1N4148"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=1 2=2"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "pwm_driver_kicad.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at -2.185 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 4.038 0 0)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at -1.8715 -0.05 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.5 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.5 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-34_SOD68_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Alps_RK163_Single_Horizontal"
		(layer "F.Cu")
		(at 108.9865 56.4)
		(descr "1110U1Q 1110TNP 1110U2A 1110U0Q Potentiometer, horizontal, Alps RK163 Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk16/rk16.pdf")
		(tags "Potentiometer horizontal Alps RK163 Single")
		(property "Reference" "RV1"
			(at 4.5 12.5 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "50k"
			(at 5.3635 5.25 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alps_RK163_Single_Horizontal"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Params" "r=50k pos=0.75"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=r0 2=wiper 3=r1"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "POT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Root")
		(sheetfile "pwm_driver_kicad.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.3135 5.1 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 3 3)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(D2-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 5 180)
			(size 3 3)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U1-THR)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 10 180)
			(size 3 3)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(D1-K)")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/pwm_driver_3d_models/potentiometer/potentiometer.step"
			(offset
				(xyz -0.75 -5 12.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 180 -90)
			)
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 117.6865 66 90)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U1"
			(at 3.95 2.7135 90)
			(layer "F.SilkS")
		)
		(property "Value" "NE555P"
			(at 3.8 4.5135 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne555.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "SUBCKT"
			(at 182.6365 -53.1965 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "${KIPRJMOD}/pwm_driver_spice_simulation_models/555.lib"
			(at 182.6365 -53.1965 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "555b"
			(at 182.6365 -53.1965 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=1 2=2 3=3 4=4 5=5 6=6 7=7 8=8"
			(at 182.6365 -53.1965 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(sheetname "Root")
		(sheetfile "pwm_driver_kicad.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.95 2.6635 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U1-THR)")
			(pinfunction "TR")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(Q1-G)")
			(pinfunction "Q")
			(pintype "output")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pinfunction "R")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(U1-CV)")
			(pinfunction "CV")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U1-THR)")
			(pinfunction "THR")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(D1-A)")
			(pinfunction "DIS")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_circle
		(center 108 77)
		(end 109.5 77)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 108 48)
		(end 109.5 48)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 137 48)
		(end 138.5 48)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 104.9865 45)
		(end 139.9865 80)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 137 77)
		(end 138.5 77)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "PWM-"
		(at 132.9865 67.75 90)
		(layer "F.SilkS")
	)
	(gr_text "PWM Driver"
		(at 122.9865 53.5 180)
		(layer "F.SilkS")
	)
	(gr_text "       -   +"
		(at 133.2365 69.75 90)
		(layer "F.SilkS")
	)
	(gr_text "Klöckner"
		(at 110.7365 78.25 0)
		(layer "F.SilkS")
	)
	(zone
		(net 8)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 104.9865 45) (xy 139.9865 45) (xy 139.9865 80) (xy 104.9865 80)
			)
		)
	)
)
